The kppp Handbook
Prev | Chapter 8. Modem Tricks and Hints | Next

# 8.4. Make Tone dialling faster

If you can use tone dialling, the amount of time it takes to dial can be changed using the `S11` register. It gives the duration (in 100hundreds of a second) to send each tone while dialling. The default is usually 95 (almost a second.) How fast you can dial depends on the phone company's switching equipment which handles your line. The minimum duration is 50, almost twice as fast, and that speed often works.

     ATZ        # reset to default profile
     ATS11=50   # fastest possible dialling, use a higher number if it doesn't work
     AT&W   # write to default profile

Prev | Home | Next
Getting the modem to hang up | Up | Configuring kppp for callback